Synchronet Bench Mark Performance Results
-----------------------------------------

System: 10mhz XT, 8bit ethernet, VGA video, DOS v3.3
Server: 16mhz 386sx, 8MB RAM, 16bit ethernet, NetWare v3.11

Test Type
-------------------------
Output (local)	       40
File Search	       46
Small Record Reading   39
Small Record Update   147
Large Record Writing   95
Large Record Reading   90

*******************************************************************************

System: 12mhz 286, 16bit ethernet, Mono video, DOS v5.0
Server: 16mhz 386sx, 8MB RAM, 16bit ethernet, NetWare v3.11

Test Type
-------------------------
Output (local)	       13
File Search	       24
Small Record Reading   17
Small Record Update    66
Large Record Writing   40
Large Record Reading   38

*******************************************************************************

System: 12mhz 286, 16bit ethernet, VGA video, DOS v5.0
Server: 8MB RAM, 16bit ethernet, NetWare v3.11

			      Servers
Test Type	    16mhz 386sx     40mhz 386
---------------------------------------------
Output (local)		22		22
File Search		22		15
Small Record Reading	18		13
Small Record Update	65		47
Large Record Writing	35		28
Large Record Reading	32		27

*******************************************************************************

System: 16mhz 386sx, 8MB RAM, 28ms ST506 MFM hard disk, SVGA video, DOS v5.0

Note:  1MB EMS cache used with Smartdrv tests

Test Type	   buffers=20	  Smartdrv 3.13   Smartdrv 4.0
-------------------------------------------------------------------------------
Output (local)	       15	       15	       15
File Search	       12	       12	       11
Small Record Reading	7		7		8
Small Record Update    23	       22	       23
Large Record Writing   63	       73	       45
Large Record Reading   25		3		4

*******************************************************************************

System: 50mhz 486, 8MB RAM, 28ms ST506 MFM hard disk, SVGA video, DOS v5.0

Note:  1MB EMS cache used with Smartdrv v3.13

Test Type
-------------------------------------------------------------------------------
Output (local)		5
File Search		2
Small Record Reading	1
Small Record Update	3
Large Record Writing   67
Large Record Reading	1

*******************************************************************************

System: 16mhz 386sx, 8bit ethernet, SVGA video, DOS v5.0, DV v2.42
Server: 16mhz 386sx, 8MB RAM, 16bit ethernet, NetWare v3.11

					--> 2 Nodes, 2nd Waiting for Keystroke
					|      (DESQview enhancement level 2)
					|
		 1 Node under <--	|	--> 2nd Node Waiting for Call
		   DESQview	|	|	|    (DV enhancement level 1)
				|	|	|
	       Normal <--	|	|	|	--> 2nd Node Uploading
Test Type		|	|	|	|	|  (DV enhance level 0)
-------------------------------------------------------------------------------
Output (local)	       15      16      17      23      33
File Search	       26      49      54      76     100
Small Record Reading   17      31      34      49      65
Small Record Update    70     111     121     179     230
Large Record Writing   44      53      57      77      97
Large Record Reading   41      51      56      76      94

*******************************************************************************

System: 50mhz 486, 8bit ethernet, SVGA video, DOS v5.0
Server: 16mhz 386sx, 8MB RAM, 16bit ethernet, NetWare v3.11

Test Type
-------------------------
Output (local)		5
File Search	       17
Small Record Reading   11
Small Record Update    48
Large Record Writing   44
Large Record Reading   42

*******************************************************************************

System: 40mhz 386, 16bit ethernet, SVGA video, DOS v5.0
Server: 16mhz 386sx, 8MB RAM, 16bit ethernet, NetWare v3.11

Test Type
-------------------------
Output (local)		5
File Search	       16
Small Record Reading   11
Small Record Update    44
Large Record Writing   30
Large Record Reading   27

